{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":4,"n_cols":12,"rows_kept":4,"merged":[[0,0,0,11],[1,0,1,6],[1,7,1,10],[1,11,2,11],[4,0,4,11],[5,7,5,9]],"flags":["formulas_cached_only"]}
["贵州锦兴轻合金装备制造有限公司招聘需求计划表"]
["需求信息",{"$nulls":6},"招聘要求",{"$nulls":3},"备注"]
["序号","用人单位","单位性质","需求部门","需求岗位","岗位数量","岗位主要职责","专业","职业资格或职称","学历学位要求","任职资格"]
["1","贵州锦兴轻合金装备制造有限公司","国有企业","模\n具\n部","修\n模\n工","2","  1、检查模具有无损坏，如裂纹，挤凹等，确定问题模具是否有利用价值，需补充的填写申请上报。\n  2、检查每块料样的检测数据，特别是关键尺寸，防止出现漏检、误检等问题。\n  3、跟踪在校正的断面，了解校正内容对模具进行调整。在模具试验合格后，要进行氮化处理。\n  4、修整模具时要了解挤压工艺执行情况，挤压设备的稳定性。对影响产量、质量的各种不利因素与料头、料样充分结合起来，总结以往修模经验确定修整方案。\n  5、监督检查模具工作带的抛光质量，组装后入库或上机使用必须保证模具内外表面的清洁。\n  6、一切工作要以生产计划为主线为挤压车间提供优质的模具，不能出现缺模现象，确保生产计划的完成。\n  7，掌握库存模具的使用情况，结合计划进行补充模具。","不限",null,"高中以上","1、3000T以上挤压机专职修模7年以上工作经验；\n2、团队意识强，沟通能力好；\n3、有吃苦耐闹的精神；能及时完成领导安排的任务，认可公司文化；\n"]